NAVSEA

STANDARD ITEM

 FY-22

 ITEM NO: 009-118

 DATE: 18 JUL 2014

 CATEGORY: I

1. SCOPE:

 1.1 Title: CG Deck Loading; accomplish

2. REFERENCES:

 2.1 671-8416047, CG47 Class Topside Laydown Areas & Load Limits

3. REQUIREMENTS:

 3.1 Accomplish the requirements of 2.1 for topside deck loading of contractor equipment and supplies.

 3.1.1 Submit one legible drawing or sketch of a proposed deck loading plan to the SUPERVISOR for review and acceptance 3 days prior to the start of the availability.

 3.1.1.1 Submit updated or changed plans to the SUPERVISOR as they occur.

4. NOTES:

 4.1 None.